|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CUTTING LIST SINGLE CAM AUTOMATA** | | | | | |
| **Material to be used** | **Name the piece** | **No of pieces** | **Length** | **Width** | **Thickness** |
| **Radiata pine** | **Base** | **1** | **70** | **50** | **19** |
| **pine** | **Sides** | **2** | **150** | **70** | **12** |
| **pine** | **Top** | **1** | **100** | **70** | **12** |
| **MDF** | **cam** | **1** | **45** | **45** | **12** |
| **pine** | **Follower** | **1** | **70** | **45** | **12** |
| **pine** | **Handle** | **1** | **50** | **20** | **12** |
| **Tas oak dowel** | **Shaft** | **1** | **120** | **6** | **6** |
| **Tas oak dowel** | **Handle** | **1** | **40** | **6** | **6** |
| **plywood** | **Washer** | **2** | **20** | **20** | **6** |
| **Tas oak dowel** | **Follower rod** | **1** | **210** | **6** | **6** |
| **pine** | **Moving figure** | **1** | **200** | **140** | **12** |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CUTTING LIST DOUBLE CAM AUTOMATA** | | | | | |
| **Material to be used** | **Name the piece** | **No of pieces** | **Length** | **Width** | **Thickness** |
| **Radiata pine** | **Base** | **1** | **150** | **70** | **19** |
| **pine** | **Sides** | **2** | **150** | **70** | **12** |
| **pine** | **Top** | **1** | **190** | **70** | **12** |
| **MDF** | **cam** | **2** | **45** | **45** | **12** |
| **pine** | **Follower** | **2** | **70** | **45** | **12** |
| **pine** | **Handle** | **1** | **50** | **20** | **12** |
| **Tas oak dowel** | **Shaft** | **2** | **120** | **6** | **6** |
| **Tas oak dowel** | **Handle** | **1** | **40** | **6** | **6** |
| **plywood** | **Washer** | **2** | **20** | **20** | **6** |
| **Tas oak dowel** | **Follower rod** | **2** | **210** | **6** | **6** |
| **pine** | **Moving figure** | **1** | **200** | **140** | **12** |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CUTTING LIST FOR LINK AUTOMATA** | | | | | |
| **Material to be used** | **Name the piece** | **No of pieces** | **Length** | **Width** | **Thickness** |
| **Radiata pine** | **Base** | **1** | **150** | **80** | **19** |
| **pine** | **Sides** | **2** | **120** | **80** | **12** |
| **pine** | **Top** | **1** | **175** | **80** | **12** |
| **pine** | **Link** | **2** | **50** | **20** | **12** |
| **pine** | **Small sides** | **2** | **105** | **40** | **12** |
| **pine** | **Handle** | **1** | **50** | **20** | **12** |
| **Tas oak dowel** | **Shaft** | **2** | **200** | **6** | **6** |
| **pine** | **Shaft extension** | **1** | **30** | **20** | **12** |
| **Tas oak dowel** | **Handle** | **1** | **40** | **6** | **6** |
| **plywood** | **Washer** | **2** | **20** | **20** | **6** |
|  |  |
| **pine** | **Moving figure** | **As required!** |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |